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Broadcast Aggregate Interior Florspartic 100 Flooring System Guideline Specification

DIVISION 09
FINISHES
PART  1  - GENERAL

1.1  
RELATED DOCUMENTS 

A.
Drawings and general provisions of the Contract, including General and Supplementary Conditions and Division 1 Specification Sections, apply to this section.

1. 2
SUMMARY

A.
Work specified in this section includes all labor, materials, equipment and services necessary to complete the proprietary Bomanite Broadcast Aggregate Flooring System including surface preparation, primers, aggregate and surface treatments.
B.
Related Sections include the following:

1. 
Division 1 Section “Product Requirements” for submittals and substitutions.

2. 
Division 3 Section “Cast-in-Place Concrete” for concrete slabs. 

3.
Division 3 Section “Joint Sealers” Installation of caulking if required
1.3
SUBMITTALS
A. 
Product Requirements:

1. 
Provide submittal information within 35 calendar days after the contractor has received the owner's notice to proceed.

B. 
Product Data:

1. 
Submit Bomanite specifications, test data and other data required for each type of manufactured material and product indicated.

2. 
Submit Bomanite Technical Bulletins listing product name, descriptive data, curing time and application requirements.

3. 
Submit Bomanite Material Safety Data Sheet (SDS) and other safety requirements.

C.
Field quality-control test and inspection reports.

1.
Documentation by the Bomanite contractor of surface profile and moisture test results prior to installation.
2.
In situ slab moisture tests resulting in a reading of 4 lbs or greater per foot in a 24 hour period or 85% relative humidity are unacceptable for this type of installation. Consult with the Bomanite installer or Bomanite Technical Services on an appropriate system designed to suppress the moisture prior to installation.
1.4
QUALITY ASSURANCE

A.
Installer Qualifications: The contractor for this work shall be a Bomanite Toppings System Licensee Licensed and Certified Applicator approved by The Bomanite Company 
(303)  369-1115 or imagine@bomanite.com. 

1.
Provide letter of certification from Bomanite Company stating that installer is a certified applicator of special concrete finishes and is familiar with proper procedures/installation requirements of the manufacturer.

2.
Use an authorized Bomanite Licensee and adequate number of skilled workmen who are thoroughly trained and experienced in the necessary craft.

3.
Applicator shall be familiar with the specified requirements and the methods needed for proper performance of work of this section.

4.
Applicator shall be familiar with the previously approved mock-ups that demonstrated standard of workmanship.

5.
Authorized Bomanite Toppings System installers limited to the following:
a.
http://bomanite.com/find-licensed-contractors/ or approved by the Bomanite Company
B.
Manufacturer Qualifications: A firm experienced in the support and training of a national installer network and manufacturing products required/listed to complete the work.

1.
Bomanite Company 303-369-1115 – no equal


C.
Source Limitations:
1.
Broadcast Aggregate Flooring System related materials: Obtain each type of material of the same brand from one source from a single manufacturer.

2.
Do not interchange manufactured materials within the Broadcast Aggregate Flooring System as all warranties whether expressed or implied will be null and void.
D.
Mock-ups:

1.
Apply finish to mock-ups constructed by Bomanite Licensed Installer, using each type of finish to demonstrate finished appearance and standard of workmanship.

a.
Mock-up shall include entire system, including surface preparation, primers, aggregate, expansion/isolation joints and surface treatments. 
b.
Notify Architect seven days in advance of dates and time when mock-ups will be constructed.

c.
Obtain from Architect approval of mock-ups before starting construction.

d.
If the Architect determines that the mock-ups do not meet requirements, General Contractor will demolish and remove them from the site and arrange to assemble more until approved.

e.
Maintain mock-ups during construction in an undisturbed condition as a standard for judging the completed work.

1.5
DELIVERY, STORAGE AND HANDLING

A. 
Deliver materials in original packages and containers, with seals unbroken, bearing Bomanite or Bomanite approved vendor labels indicating brand name and directions for storage, mixing with other components and application.

B. 
Store materials to comply with Bomanite written instructions to prevent deterioration from moisture or other detrimental effects.

C. 
Dispense special concrete finish material from Bomanite factory numbered and sealed containers. Maintain record of container numbers.

1.6
PROJECT CONDITIONS

A. 
Environmental Limitations:

1.
Comply with Bomanite written instructions for ambient temperature and other conditions affecting installation performance.

2. 
Concrete must be cured a minimum of 28 days or as directed by the manufacturer before installation of Bomanite Broadcast Aggregate Flooring System can begin.

1.7
PERFORMANCE REQUIREMENTS

A. The product is required to resist water intrusion indefinitely provided no structural movement has compromised the system.
B. The product is required to have a clear non-yellowing high-performance coating applied as a topcoat with a non-slip finish.
C. The product is required to have resistance to common solvents.
D. The product is required to be comprised of Polyaspartic polymers and curatives. 
PART  2  - PRODUCTS

2.1  
MANUFACTURERS 

A.
In other Part 2 articles where titles below introduce products, the following requirements apply to product selection:

1.
Available Manufacturers: Subject to compliance with requirements, manufacturers offering materials required to be incorporated into the work include, and are limited to, manufacturer listed. 


a. The Bomanite Company (303) 369-1115 www.bomanite.com 
2.2
MATERIALS
A. 
Bomanite Florspartic 100 Gloss: A topically applied 100% solids Polyaspartic coating designed to be applied to correctly prepared wood, concrete and engineered cementitious products along with manufacturer approved epoxies.  
B. 
Broadcast Aggregate: Factory colored and field blended quartz aggregates. 
C.
No substitutions or alternates to the above will be accepted.

PART 3 – EXECUTION

3.1
EXAMINATION
A.
Consult General Contractor, Structural Engineer, Architect and Concrete Contractor with Bomanite installer present prior to pouring the concrete slab to which the Bomanite Broadcast Aggregate Flooring System is to be applied to. Ensure complete understanding of substrate preparation, vapor barrier installation, control joint placement, penetrations, mechanical bases, slope to drains etc. 
B.
Examine slab prior to installation with Bomanute installer present for conditions affecting performance of the Bomanite Broadcast Aggregate Flooring System. Rectify conditions detrimental to timely and proper work . Do not proceed with installation of Bomanite Broadcast Aggregate Flooring System until unsatisfactory conditions are corrected.
C.
Repair of defective portions of concrete slab due to improper installation is the responsisbility of the Bomanite installer. All repairs must meet the satsifaction of the architect.
3.2
SURFACE PREPARATION
A.
Mechanically profile the concrete slab with planetary head grinders and hand held grinders to International Concrete Repair Institute Concrete Surface Profile 2 standards or greater. 
B.
Treat all cracks and control joints with a semi-rigid penetrating polyurea or equal two component product in a manner consistent with the repair product manufacturer’s guidlines. Grind the repair flush to the concrete slab prior to the Bomanite Broadcast Aggregate Flooring System installation.
C.
Construction and Contraction/Expansion/Isolation Joints:

1.
Clean joints mechanically using hand held or walk behind grinders with crack chasing type blade after substantial completion of  the Bomanite Broadcast Aggregate Flooring System.

2.
Fill all joints with  a shore 40 A polyurea or polyurethane joint filler in a manner consistent with the repair product manufacturer’s guidlines.
3.3
INSTALLATION
A.
Apply the Bomanite  Broadcast Aggregate Flooring System according to the manufacturers proprietary internal application procedures including  prime coats, pigmented basecoats, aggregate, clear topcoat and joint fillers.
B.
Coat perimeter of room and mechanical bases a minimum of 4” up the vertical faces (optional and requires the use of preformed cove base).  

3.4
PROTECTION

A. It is the General Contractor’s responsibility to provide and install protection according to Bomanite installer’s recommendations. Protection of the finished surface is to be maintained by the General Contractor until substantial completion of the project is met and the floor can go into service. 

END OF SECTION
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International Society

OVER 225 CONTRACTORS WORLDWIDE

The Bomanite International Society of licensed contractors is a worldwide network of specially trained and equipped professionals. Through constant exchange of new ideas, re-education and development programs, members of the Bomanite International Society continue to increase already high standards of quality and service. The activities of the Bomanite International Society are coordinated by The Bomanite Company. The Corporation also provides services and technical assistance to its member Licensed Contractors, and to architects, designers and engineers specifying Bomanite products. For more information, including a list of members of the Bomanite International Society, contact:

Bomanite LLC
34501 East Quincy Ave. Building 28
Watkins, CO 80137
Tel: (303) 369-1115
Fax: (303) 291-0282
Web site: www.bomanite.com 

Email: imagine@bomanite.com 
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